|  |  |  |  |
| --- | --- | --- | --- |
| **Sr. No.** | **Part/Material** | **Specification/Dimensions** | **Requirement** |
| 1 | Pedestal Bearing | UC 201 | 2 Nos |
| 2 | Flat Plate | 150\*40\*3 mm | 2 Nos |
| 3 | L channel | 25\*25\*2 | 8 Feet |
| 4 | Shaft | Φ 12 mm | 500 mm |
| 5 | Punched Mesh | 1 mm thick | 2\*3 feet |
| 6 | MS Sheet | 0.8 mm thick | 5\*1 feet |
| 7 | Nut Bolt | M12\* 50 mm | 4 Nos |
| 8 | Trey | 430\*310\*70 mm | 1 No |

**MATERIAL REQUIREMENT FOR DOMESTIC COMPOSTER**